(footprint "LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
	(tags "LED RGB NeoPixel PLCC-4 5050")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
		(uuid "61c09ae9-d011-4856-9faf-1d71dd92e2d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WS2812B"
		(at 0 4 0)
		(layer "F.Fab")
		(uuid "bac1306f-1cd2-42f7-8020-5d1101447b6b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "411a61a6-4728-492c-8ce7-b58702779839")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "RGB LED with integrated controller"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcac83ae-aaad-48e6-be53-66d1e7e66899")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.5 -2.75)
		(end -3.5 2.75)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e54ef800-f483-44d4-8882-70da325234ff")
	)
	(fp_line
		(start -3.5 -2.75)
		(end 3.5 -2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "094d5d21-83f9-44db-8c57-72fda88f63b4")
	)
	(fp_line
		(start -3.5 2.75)
		(end 3.05 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1bf48fb2-28c4-4254-8842-737dd676c83e")
	)
	(fp_line
		(start -2.7 0.9)
		(end -2.7 -0.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6c2200a5-8171-4737-927d-1d311f7de40b")
	)
	(fp_line
		(start 2.7 0.9)
		(end 2.7 -0.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c3e19b03-b218-42c5-b531-23bbdf6fa454")
	)
	(fp_line
		(start 3.05 2.75)
		(end 3.5 2.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "de88a3ae-3ea4-40c4-9950-900ca7e67249")
	)
	(fp_line
		(start 3.5 2.3)
		(end 3.5 -2.75)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "118d6367-d0ca-4d32-9f78-fab3678d7abf")
	)
	(fp_line
		(start -3.45 -2.75)
		(end -3.45 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e986a1b-7128-4d4c-adc9-0b6bba670005")
	)
	(fp_line
		(start -3.45 2.75)
		(end 3.45 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fec726d0-defd-4924-8112-de303a717b08")
	)
	(fp_line
		(start 3.45 -2.75)
		(end -3.45 -2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2db57d0a-5abe-4b8e-9319-183fa27bfd02")
	)
	(fp_line
		(start 3.45 2.75)
		(end 3.45 -2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c0eb440e-1ba4-4cbb-ad42-a73b55c138dc")
	)
	(fp_line
		(start -2.5 -2.5)
		(end -2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "541ead05-e313-4936-bc6c-ae757b8e37a2")
	)
	(fp_line
		(start -2.5 2.5)
		(end 2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "564ae1be-5ef4-4750-b515-0382ed21c639")
	)
	(fp_line
		(start 2.5 -2.5)
		(end -2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1296a15d-9b58-4628-b979-212f7658d3ba")
	)
	(fp_line
		(start 2.5 1.5)
		(end 1.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5bbb876a-fd12-4f01-8c1b-c0318070a2ec")
	)
	(fp_line
		(start 2.5 2.5)
		(end 2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dd08dc92-6cc3-4cde-8a4e-cf225170b610")
	)
	(fp_circle
		(center 0 0)
		(end 0 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "66a5099b-1235-47bc-b72f-8e0bdf31f12c")
	)
	(fp_text user "1"
		(at -4 -1.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ee1dd1d3-2d86-469e-894c-ac1ab430d43b")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "f11e2144-4dca-428a-b4a0-c181af4a4f70")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.45 -1.65)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "46229028-d109-438b-bd00-f3f093ac8224")
	)
	(pad "2" smd roundrect
		(at -2.45 1.65)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "5d2dd6a1-bb99-43d0-9b40-98a73d0db8f3")
	)
	(pad "3" smd roundrect
		(at 2.45 1.65)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "cb2ce687-051d-4178-8eae-5a8983725408")
	)
	(pad "4" smd roundrect
		(at 2.45 -1.65)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "129a9e22-d47e-4b1a-ba1a-1587f60b6ffb")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
