(footprint "RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Alps rotary encoder, EC11E... with switch, vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
	(tags "rotary encoder")
	(property "Reference" "REF**"
		(at 2.8 -4.7 180)
		(layer "F.SilkS")
		(uuid "feb12d80-9d08-42da-917b-bf58cdc9b7de")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "RotaryEncoder_Switch"
		(at 7.5 10.4 180)
		(layer "F.Fab")
		(uuid "6b84f501-0bd7-4277-8b25-9df1237567fa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "~"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "46264c5d-1522-45ca-8904-efcfd2985ca0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "085c446d-823b-4b21-a520-989fa88a68b9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -0.3 -1.6)
		(end 0.3 -1.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "72872d2c-55f4-491a-883c-5b463b8902e1")
	)
	(fp_line
		(start 0 -1.3)
		(end -0.3 -1.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8a7d1cfd-56c7-49a8-a472-1100bec07ea3")
	)
	(fp_line
		(start 0.3 -1.6)
		(end 0 -1.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3f2b8212-55f6-46ca-964a-af30dce65e5a")
	)
	(fp_line
		(start 1.4 -3.4)
		(end 1.4 8.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7a9f3d4e-90f1-4031-9286-d5be5de5a46c")
	)
	(fp_line
		(start 5.5 -3.4)
		(end 1.4 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "409ceaa5-b666-44da-b8b7-8e25f108a65f")
	)
	(fp_line
		(start 5.5 8.4)
		(end 1.4 8.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2f280768-2a4a-496b-ab30-63bd2a264f82")
	)
	(fp_line
		(start 7 2.5)
		(end 8 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "96f2f735-1beb-4817-89e9-c5be36f602bc")
	)
	(fp_line
		(start 7.5 2)
		(end 7.5 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "82af04a8-0069-4f92-9f45-201ab3c8b118")
	)
	(fp_line
		(start 9.5 -3.4)
		(end 13.6 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de2885da-cda9-45c2-b63b-568e4068a8ef")
	)
	(fp_line
		(start 13.6 -3.4)
		(end 13.6 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3eeb6266-8bd0-4268-9733-c5e35dc6ffda")
	)
	(fp_line
		(start 13.6 1.2)
		(end 13.6 3.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0d3a83f6-4c5a-405f-94fb-de9720faf66b")
	)
	(fp_line
		(start 13.6 6)
		(end 13.6 8.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c6b5cc1e-be03-4230-89c5-f61a183da573")
	)
	(fp_line
		(start 13.6 8.4)
		(end 9.5 8.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "446cf392-6bec-48f8-8da9-75e845747baf")
	)
	(fp_circle
		(center 7.5 2.5)
		(end 10.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "7d59ef10-e17f-4bcf-a783-83e03991a1d4")
	)
	(fp_line
		(start -1.5 -4.6)
		(end -1.5 9.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99cf83f8-3e34-46dc-9bfa-73a25ed049af")
	)
	(fp_line
		(start -1.5 -4.6)
		(end 16 -4.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "714327b5-1a44-4b85-b063-b38979fdfa26")
	)
	(fp_line
		(start 16 9.6)
		(end -1.5 9.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c5f42bcf-cedd-4f1e-80f0-278880e6238b")
	)
	(fp_line
		(start 16 9.6)
		(end 16 -4.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "279f6722-47ca-44da-9573-040a09e7169a")
	)
	(fp_line
		(start 1.5 -2.2)
		(end 2.5 -3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "75ed5c3f-0243-4a70-bd4f-05550ccc923a")
	)
	(fp_line
		(start 1.5 8.3)
		(end 1.5 -2.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7b080f8f-d60c-42a2-a63d-7d4f076c39b6")
	)
	(fp_line
		(start 2.5 -3.3)
		(end 13.5 -3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "14d0f0fe-65ff-4139-86f6-aadfabc9e16c")
	)
	(fp_line
		(start 4.5 2.5)
		(end 10.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "924a40d9-93d7-4c68-9cd4-964da5e6c747")
	)
	(fp_line
		(start 7.5 -0.5)
		(end 7.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "51c40b78-d059-45aa-9c7f-e61f815f089d")
	)
	(fp_line
		(start 13.5 -3.3)
		(end 13.5 8.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d46c8270-840a-48cf-bfc9-f1f1c90fabcf")
	)
	(fp_line
		(start 13.5 8.3)
		(end 1.5 8.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ce228c7f-9885-4ea7-8535-53cf90f3e880")
	)
	(fp_circle
		(center 7.5 2.5)
		(end 10.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "7edeb939-87e7-4a1a-814c-673719f6d7e8")
	)
	(fp_text user "${REFERENCE}"
		(at 11.1 6.3 180)
		(layer "F.Fab")
		(uuid "bae60c76-061b-4f18-b4f3-89724a8eed75")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "A" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7e5a8d53-eaf3-4bc9-9c72-aa53631ca59c")
	)
	(pad "B" thru_hole circle
		(at 0 5)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5797fde2-7f2d-4ea1-ac0a-d6ff2a64989d")
	)
	(pad "C" thru_hole circle
		(at 0 2.5)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6752182d-8b1c-4726-80c2-a1a071bb2bfb")
	)
	(pad "MP" thru_hole rect
		(at 7.5 -3.1)
		(size 3.2 2)
		(drill oval 2.8 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6d818e60-ea6d-47be-ad19-b2f5fdf2b4ba")
	)
	(pad "MP" thru_hole rect
		(at 7.5 8.1)
		(size 3.2 2)
		(drill oval 2.8 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5f009c64-0a6b-4f00-afd8-56872e721f12")
	)
	(pad "S1" thru_hole circle
		(at 14.5 5)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b907227-0863-4095-87d5-1ea9580495ea")
	)
	(pad "S2" thru_hole circle
		(at 14.5 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b0457e2c-4ebe-4ef4-83f9-f41c6bb1f446")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
