(footprint "R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
	(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
	(property "Reference" "REF**"
		(at 3.81 -1.92 0)
		(layer "F.Fab")
		(uuid "894f5285-48a6-42c6-a2ca-cdcdf779b114")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "4.7k"
		(at 3.81 0 0)
		(layer "F.SilkS")
		(uuid "9ffd4bd3-aec8-4920-8f9f-5a135d629e74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.vishay.com/docs/20035/dcrcwe3.pdf"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9bf73a82-75b0-4f31-9612-f58d3cf8eeff")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Resistor"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "5dccd662-e7c3-417b-8327-69a4ff066ef6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "PROD_ID" "RES-00824"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6660a778-99d3-4721-9de3-9c14d3809ac1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 0.94 0)
		(end 1.89 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "01e13a5c-47ed-41f4-8273-a4d9572bb72e")
	)
	(fp_line
		(start 6.68 0)
		(end 5.73 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6b15b6e9-2516-4b12-bcb5-fef378db86e0")
	)
	(fp_rect
		(start 1.89 -0.92)
		(end 5.73 0.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "8abf5ca3-e54e-43d2-aa76-9fc0efa996e1")
	)
	(fp_rect
		(start -0.95 -1.05)
		(end 8.57 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "5f6d9a5a-218e-47ba-a5e3-96800d9d5408")
	)
	(fp_line
		(start 0 0)
		(end 2.01 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "504b097e-f215-41d1-816c-b398eca63399")
	)
	(fp_line
		(start 7.62 0)
		(end 5.61 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "54ab655c-150b-478c-b97d-a9529e9aa4ac")
	)
	(fp_rect
		(start 2.01 -0.8)
		(end 5.61 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "683ec57e-7db0-46b4-8783-d50c12db1b4a")
	)
	(fp_text user "${REFERENCE}"
		(at 3.81 0 0)
		(layer "F.Fab")
		(uuid "3b4a91ea-314a-47ba-b7fc-c11ecc01d405")
		(effects
			(font
				(size 0.72 0.72)
				(thickness 0.108)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "00eac638-2f64-4116-8f2a-9090775c3fcd")
	)
	(pad "2" thru_hole circle
		(at 7.62 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "10f24769-f63e-458f-a91e-612aa9869b02")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
