(footprint "gateron-ks27-choc-v1-mx-soldered"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.1 -8.5 180)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c407c363-ee0c-42b2-ac0d-3383b9a81edb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_FSkey"
		(at 0 8.5 180)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6e94b3b4-3004-4732-853f-33e92638be39")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "~"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f7ae708a-1506-45e4-825e-b19232f02852")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Push button switch, generic, two pins"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7313edfe-e788-4670-aad9-c74ef9bf11e4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 7 7)
		(end 7 -7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "10e54ec8-0ed0-4245-b0c6-fc8963bc1f34")
	)
	(fp_line
		(start 7 -7)
		(end -7 -7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "190c59ef-c028-4557-b390-713925896559")
	)
	(fp_line
		(start -7 7)
		(end 7 7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "8091563c-7d22-4ff3-b6a5-2616f841192e")
	)
	(fp_line
		(start -7 -7)
		(end -7 7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Eco2.User")
		(uuid "de231cb7-d7d6-4947-8786-643eb3003586")
	)
	(fp_line
		(start 3.81 6.985)
		(end -5.08 6.985)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.Fab")
		(uuid "1fe1f679-0b5d-43c6-be1d-acda219fde41")
	)
	(fp_line
		(start 7.5 7.5)
		(end 7.5 -7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e4babcaa-6c65-4a24-9820-25685ee08862")
	)
	(fp_line
		(start 7.5 -7.5)
		(end -7.5 -7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0456f901-fe09-42a5-8378-d04734c54c4f")
	)
	(fp_line
		(start -7.5 7.5)
		(end 7.5 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3105c328-88ca-430e-b078-d0222c3073a5")
	)
	(fp_line
		(start -7.5 -7.5)
		(end -7.5 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6570885-2770-496f-954d-762c32899e45")
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 -8.5 0)
		(layer "B.Fab")
		(uuid "e82ac912-7643-48f2-b984-ba6d6ebccd67")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(pad "" np_thru_hole circle
		(at -5.5 0 180)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "f9fe94fe-ef92-471d-b2e5-05904d8a3725")
	)
	(pad "" np_thru_hole circle
		(at -5.08 0)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "2500bbbf-7b8e-4422-9b3f-a78d9a151657")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 3.9878 3.9878)
		(drill 3.9878)
		(layers "*.Cu" "*.Mask")
		(uuid "1e347234-b10d-4a56-82d2-e3047cc25f34")
	)
	(pad "" np_thru_hole circle
		(at 0 0 180)
		(size 5 5)
		(drill 5)
		(layers "*.Cu" "*.Mask")
		(uuid "fdc8074b-2a4b-432d-ab7c-1ed9ac06df55")
	)
	(pad "" np_thru_hole circle
		(at 5.08 0)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "5dfc5bc2-b136-4441-a1d3-7bd388d11929")
	)
	(pad "" np_thru_hole circle
		(at 5.5 0 180)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "608a5efa-b96a-4a8e-b9ee-13921a8179f3")
	)
	(pad "1" thru_hole circle
		(at -5 -3.8)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a93d0952-967a-4cdb-8d7f-6fbd56834257")
	)
	(pad "1" thru_hole circle
		(at -4.4 -4.7)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a6e50984-d02a-4878-ab8f-0d83320e7789")
	)
	(pad "1" thru_hole circle
		(at -2.54 -5.08)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f6389d2d-0548-40ac-9934-f637e64d29ae")
	)
	(pad "2" thru_hole circle
		(at 0 -5.9)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "300c68f5-5702-4ac1-ba52-167029135725")
	)
	(pad "2" thru_hole circle
		(at 2.6 -5.75)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2aaa1006-f123-4e64-8918-4f49f16c76a4")
	)
	(pad "2" thru_hole circle
		(at 3.81 -2.54)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1aeb71bc-86fe-44fd-b726-f2e008d69b14")
	)
	(embedded_fonts no)
)
