(footprint "R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
	(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
	(property "Reference" "REF**"
		(at 2.54 -1.92 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "17324fc3-256a-4ac6-9948-b74aa0d5120f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "4.7k"
		(at 2.54 0 180)
		(layer "F.SilkS")
		(uuid "3f1c95d4-e8c7-4a6a-b2e7-677eee414979")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "~"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "87a867f7-4ea7-453e-9d7a-670851fcd82a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Resistor"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "9166ae82-d4b9-4bf9-8b35-141266fefea1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 0.62 -0.92)
		(end 4.46 -0.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e307e6a7-a93a-4c64-84ef-457409e026a2")
	)
	(fp_line
		(start 0.62 0.92)
		(end 4.46 0.92)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7551e224-6952-4a7f-9c61-a29b0316236c")
	)
	(fp_rect
		(start -0.95 -1.05)
		(end 6.03 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "3c4d7809-cb7f-4a1d-8604-6e567b9950b1")
	)
	(fp_line
		(start 0 0)
		(end 0.74 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f53a676c-2db8-4a70-8762-8489220407f6")
	)
	(fp_line
		(start 5.08 0)
		(end 4.34 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d856d18-495e-4a94-9ef0-07edbb5c4386")
	)
	(fp_rect
		(start 0.74 -0.8)
		(end 4.34 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "f8cb5cf0-acd5-41f7-98a6-5ad5f45211f2")
	)
	(fp_text user "${REFERENCE}"
		(at 2.54 0 180)
		(layer "F.Fab")
		(uuid "a4d6b1e1-a33b-4908-aa15-dec390bc1db7")
		(effects
			(font
				(size 0.72 0.72)
				(thickness 0.108)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0789b5e6-51de-4ff0-bf9c-9949fd214209")
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "689b1f98-4ee4-455b-a900-6c869519fc87")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
