(footprint "C_0603"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at -0.3 -1.7 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "b6fbfa18-998f-4ed4-83db-f24590952a75")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "100nF"
		(at 0 1.43 0)
		(layer "F.Fab")
		(uuid "12e9e64e-fc34-484f-9186-7354d581cfb6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2211101700_YAGEO-CC0603KRX7R9BB104_C14663.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c988a257-2911-4017-90aa-26dbb719c5b1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "100nF 50V X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2353ece3-1da4-4ee9-8e7c-a9eb1e6f0951")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C14663"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5d22886f-0427-41a4-93fb-cd1dc156b5b8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Stock" "39955997"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6c0fa8dc-97cd-424b-9a22-1940db134ed4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Price" "0.006USD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4e0bcbba-ae9e-4fda-8c5e-b22e4c1b4e36")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Process" "SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d9c945e1-ff40-4e2b-a13e-ec54c209456f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Minimum Qty" "20"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fbe14d38-a6d4-4aba-a1e4-e6ed603ce151")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Attrition Qty" "10"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "885fc0cd-e5b5-4990-9d34-6037c634ea42")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Class" "Basic Component"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3c4ca1da-b3b4-4d4b-acd5-35788730ba88")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Category" "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "349a3c21-37b4-4e30-9d8b-fa16ce8256eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "YAGEO"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "024deb32-ffd4-4507-89e3-b6f207f7f133")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part" "CC0603KRX7R9BB104"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0eb0213c-5a64-4f47-b6b2-83e8d2700e08")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Voltage Rated" "50V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a2c3dc97-acc7-41f6-8257-048e06a7804b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Tolerance" "±10%"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "27d4bd62-609b-4647-862f-edbb5b4a6241")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Capacitance" "100nF"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "46df1771-52e3-426e-a87e-67d14e972746")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Temperature Coefficient" "X7R"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "571fd1e0-4b63-4ef7-a156-265cee34c5ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.038)
	(attr smd)
	(fp_line
		(start -1.4 -0.6)
		(end 1.4 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "919a10e9-3e63-4d77-a925-15598484bdb1")
	)
	(fp_line
		(start -1.4 0.6)
		(end -1.4 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8a84dffe-e6d2-4163-97e1-4deef42ad555")
	)
	(fp_line
		(start 1.4 -0.6)
		(end 1.4 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "816e94ec-5272-4634-9971-3fa2303ad520")
	)
	(fp_line
		(start 1.4 0.6)
		(end -1.4 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "171f2cc5-04b9-4ea0-8bde-31a008d24d43")
	)
	(fp_line
		(start -0.8 -0.4)
		(end 0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "16a04a86-199a-47df-832f-ee5f2cdd605b")
	)
	(fp_line
		(start -0.8 0.4)
		(end -0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d0d7d4f-275b-44e7-a8c7-6656bbbb1124")
	)
	(fp_line
		(start 0.8 -0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7e03b5df-ac2b-4b64-8baf-f93c42f14555")
	)
	(fp_line
		(start 0.8 0.4)
		(end -0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "237b36a8-37ae-4e95-b86a-438f264f288d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "bd5c4ae2-9e5e-4ffa-ac57-29990a07dba9")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.78 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e51c00fc-cf7c-4004-af94-279ffec32369")
	)
	(pad "2" smd roundrect
		(at 0.78 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "3c173c58-8b4c-4679-a854-14dc4d1e8273")
	)
	(embedded_fonts no)
	(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB.3dshapes/C_0603.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
