(footprint "SSD1306_I2CBreakout"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.75 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7dc032fc-322a-403a-aa93-b3c6fd62fab0")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "~"
		(at 0 -2.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9fbd2815-b03d-444b-a258-f010a52b59a1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f32c326d-b421-4630-927a-4b5c637f8d4f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c49c9ed0-e1ec-472c-b880-f8976e724e8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -12.5 -33.02)
		(end 12.5 -5.52)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "62fed9cf-12ee-4643-a014-d80775fd3fd3")
	)
	(fp_text user "SDA"
		(at 3.81 -26.67 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0ca0ad4d-d79d-47ce-9861-1b433c1bdfd5")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(fp_text user "GND"
		(at -3.81 -26.67 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "574d9073-2264-461b-b76d-f1bdc81d38e1")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(fp_text user "SCK"
		(at 1.27 -26.67 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9b2dd698-e3ac-4f6e-ba08-e2faa8d1df32")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(fp_text user "VDD"
		(at -1.27 -26.67 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c0ea5c5e-a785-4533-b733-3ede30d8c077")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.3)
				(bold yes)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3770e48f-02c5-4789-8428-2d89f457c652")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text_box "SSD1306\ni2c OLED\nScreen"
		(start -5.08 -20.32)
		(end 5.08 -10.16)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "F.SilkS")
		(uuid "9b7ae392-2d76-459c-9dbf-3470e615c6f8")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify top)
		)
		(border yes)
		(stroke
			(width 0.1)
			(type solid)
		)
	)
	(pad "1" thru_hole roundrect
		(at -3.81 -30.48 90)
		(size 2.54 1.27)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "70b326de-b285-4953-9104-0ac0f6ca0e45")
	)
	(pad "2" thru_hole roundrect
		(at -1.27 -30.48 90)
		(size 2.54 1.27)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "1bc2f6a9-e030-4b96-9777-77c2ffc94ac6")
	)
	(pad "3" thru_hole roundrect
		(at 1.27 -30.48 90)
		(size 2.54 1.27)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "af6aed34-960a-4405-9484-1b57a9319768")
	)
	(pad "4" thru_hole roundrect
		(at 3.81 -30.48 90)
		(size 2.54 1.27)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "490fd669-324d-4756-ad4b-9af96d4813c7")
	)
	(embedded_fonts no)
)
