(footprint "WeAct_PCM5100A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "40e23218-f12a-411a-8c0a-50765d029b61")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "WeAct_PCM5100A"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1dc6b840-eabc-4d02-bf61-5771773f14a3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ff7be56a-5ed1-4fc4-8ebb-3d6cd5488d28")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8214bdd4-5908-46c2-b52a-2e817d8d021e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -9.12 -21.82)
		(end -9.12 -3.58)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8f530ab2-e4c1-4067-897e-53b4d6384ec9")
	)
	(fp_line
		(start -9.12 -3.58)
		(end 0 -3.58)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bc9bf74d-e38f-4874-8f33-92c9c7a16f50")
	)
	(fp_line
		(start 0 -21.82)
		(end -9.12 -21.82)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cf22d9e8-6889-4a57-ae00-c4112cecd215")
	)
	(fp_line
		(start 0 -3.58)
		(end 9.5 -3.58)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5c791808-46ed-4a7f-9936-1ee90d75baa7")
	)
	(fp_line
		(start 9.5 -21.82)
		(end 0 -21.82)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fcb79c5e-a29d-4dd5-9f6f-ecab4a10296c")
	)
	(fp_line
		(start 9.5 -3.58)
		(end 9.5 -21.82)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "383aa4b1-a89b-48fc-8c5b-b54161fdc93f")
	)
	(fp_text user "R+"
		(at 4.5 -19.8 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "08bc01dc-2113-44f7-b889-6319b9d0fcc7")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "BCK"
		(at -6.3 -9.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0c7ab2d3-1328-42b1-a876-502c8b2a8791")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "L-"
		(at 4.6 -12.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "301497e3-3f22-4f02-a6a3-1cc405562030")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "MC"
		(at -6.3 -12.2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3950d96a-4948-4884-933e-9114d17b3049")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "WeAct PCM5100A + PA"
		(at 1.8 -3.58 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "545bf98b-1382-487a-95f9-5c0ef618e020")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "SD"
		(at -6.1 -14.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5fc39de7-5305-4912-95f8-a9090be7c5fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at -6.1 -17.2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "75e67f47-243a-4027-912e-eee4f67940f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "DIN"
		(at -6.3 -7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9c434dd6-f557-48ae-9d3b-50409a8d672a")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "L+"
		(at 4.6 -14.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "bfc844e0-54f7-4e86-8fd9-63af2ff70b39")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "VCC"
		(at -6.1 -19.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "cc6ef6ec-db74-483e-888f-3372a25099b2")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "R-"
		(at 4.5 -17.2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e85110a8-3fc4-4a8f-be75-230e14c5338d")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "WS"
		(at -6.2 -4.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f6c1530e-a9d1-43eb-b66f-b6a6dc68c970")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "53f613cb-3103-49b9-9bb8-988ef88d0056")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at -7.62 -20.32)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "85b16b48-b7af-427c-ae12-1d18472ecc39")
	)
	(pad "2" thru_hole roundrect
		(at -7.62 -17.78)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "07d33a45-4e55-49ac-9153-72f1b55ca992")
	)
	(pad "3" thru_hole roundrect
		(at -7.62 -15.24)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "960c2814-a4cc-4ffd-a8bb-96de254ed6ca")
	)
	(pad "4" thru_hole roundrect
		(at -7.62 -12.7)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "4fdebb1f-fdca-401a-b2e0-f9bb8d79f58e")
	)
	(pad "5" thru_hole roundrect
		(at -7.62 -10.16)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "1080fd36-3eea-42bc-8e17-0b265687790b")
	)
	(pad "6" thru_hole roundrect
		(at -7.62 -7.62)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "b67246cb-b863-410c-a655-ee697ae89bf7")
	)
	(pad "7" thru_hole roundrect
		(at -7.62 -5.08)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "f52fc046-b45a-4efe-b91a-3c5db1829b91")
	)
	(pad "8" thru_hole roundrect
		(at 8 -20.32)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "e306cfe3-2ea6-4700-be09-87a0c82f2337")
	)
	(pad "9" thru_hole roundrect
		(at 8 -17.78)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "6fb338fd-87a5-4f28-be40-0543dddcd47c")
	)
	(pad "10" thru_hole roundrect
		(at 8 -15.24)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "b0ed855d-2b37-4f4a-8001-4b87edad97d8")
	)
	(pad "11" thru_hole roundrect
		(at 8 -12.7)
		(size 2.54 1.27)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15)
		(uuid "09277480-1651-40a2-afc1-3df8f321b0bd")
	)
	(embedded_fonts no)
)
