(footprint "D_DO-35_SOD27_P7.62mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, length*diameter=4*2mm^2, http://www.diodes.com/_files/packages/DO-35.pdf")
	(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
	(property "Reference" "REF**"
		(at 4.25 0 180)
		(layer "F.SilkS")
		(uuid "10d5d286-828d-45cf-a57a-0ea7902ab576")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1N4148"
		(at 3.81 2.12 180)
		(layer "F.Fab")
		(uuid "485a6244-53f4-4648-9d75-0023f6727b69")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "c25a95ea-3410-41d5-8b5b-c470180d1be1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "100V 0.15A standard switching diode, DO-35"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "893e7674-c7ed-4aa5-b763-785e6a866a9b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" "D"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d7dfc359-caae-4af2-aa57-03fc452a4c4c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" "1=K 2=A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1370bf5c-c758-4865-ba03-cef5fd0d1f2a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 1.04 0)
		(end 1.69 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a180553-07f4-47d5-9cb2-a45dc4aa2a05")
	)
	(fp_line
		(start 2.29 -1.12)
		(end 2.29 1.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "89906ffd-c41a-4873-9c6d-291bb9bbac70")
	)
	(fp_line
		(start 2.41 -1.12)
		(end 2.41 1.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1911daca-1974-4565-abf4-061b611bec63")
	)
	(fp_line
		(start 2.53 -1.12)
		(end 2.53 1.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a8cff585-cb67-48e2-9aec-bcc7bb311c57")
	)
	(fp_line
		(start 6.58 0)
		(end 5.93 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aa369a37-5b23-4ff5-8514-6d0559b9460f")
	)
	(fp_rect
		(start 1.69 -1.12)
		(end 5.93 1.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "c83ce220-79bd-4398-ab69-349e52bdafb5")
	)
	(fp_rect
		(start -1.05 -1.25)
		(end 8.67 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "ca96c4a4-844b-4098-8645-ceaf911ac5df")
	)
	(fp_line
		(start 0 0)
		(end 1.81 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "215323a5-5e8f-4fa6-81b5-36708fe3b568")
	)
	(fp_line
		(start 2.31 -1)
		(end 2.31 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "64d2ec88-4438-4459-952e-f7cd5169d411")
	)
	(fp_line
		(start 2.41 -1)
		(end 2.41 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "63b4f768-d738-4d20-8a0f-af30bde87ff6")
	)
	(fp_line
		(start 2.51 -1)
		(end 2.51 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "24f653ee-3146-49d3-b829-da2a47f20a47")
	)
	(fp_line
		(start 7.62 0)
		(end 5.81 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "655dbf58-7e99-4bf7-a097-aa5f9a74f04a")
	)
	(fp_rect
		(start 1.81 -1)
		(end 5.81 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "d0bf0bb6-adbc-4e5f-99c7-98aa63a54582")
	)
	(fp_text user "K"
		(at 0 -1.8 180)
		(layer "F.Fab")
		(uuid "67549123-1904-467c-8112-eef5e715317a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 4.11 0 180)
		(layer "F.Fab")
		(uuid "783edd08-c9dc-46bb-a537-b69206e80305")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15625)
		(uuid "d9cce80e-dce0-4b43-a8bb-14ed4b286ba7")
	)
	(pad "2" thru_hole circle
		(at 7.62 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "45fa8d7a-45d4-43df-b66e-15b307b934d7")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
