(footprint "SW_PUSH_6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Generic 6mm SW tactile push button")
	(tags "tact sw push 6mm")
	(property "Reference" "REF**"
		(at 3.25 -2 0)
		(layer "F.SilkS")
		(uuid "d275afe8-596f-4a39-a451-bb67c42ffa7a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_Right"
		(at 3.75 6.7 0)
		(layer "F.Fab")
		(uuid "98f8426a-a187-4f13-acee-bfe8cca8a0c7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "~"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4961e93d-52d1-4fe5-b61a-b1f8e616f9a4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Push button switch, generic, two pins"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ec490aaa-266f-4aea-971f-dee4900e32a6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -0.25 1.5)
		(end -0.25 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca0e4096-c6f8-44d1-8014-51d88431a97c")
	)
	(fp_line
		(start 1 5.5)
		(end 5.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "86cb1744-04d8-4355-937b-3572ee75a761")
	)
	(fp_line
		(start 5.5 -1)
		(end 1 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4a005d25-e114-4e61-9474-721ef43fc646")
	)
	(fp_line
		(start 6.75 3)
		(end 6.75 1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "68685226-78bf-47ba-a03a-e9134b895ff9")
	)
	(fp_line
		(start -1.5 -1.5)
		(end -1.25 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1161d580-e804-4ac4-a571-a5ee6fb5d394")
	)
	(fp_line
		(start -1.5 -1.25)
		(end -1.5 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "14327f00-bdce-4a2b-890e-5b54bf76944e")
	)
	(fp_line
		(start -1.5 5.75)
		(end -1.5 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "81ba0c9d-e179-4cdb-9d8b-64e23896a7e2")
	)
	(fp_line
		(start -1.5 5.75)
		(end -1.5 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b32b6299-0e22-4bbb-ba14-53dc1b4dbc64")
	)
	(fp_line
		(start -1.5 6)
		(end -1.25 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "798e5180-1df5-4b47-a0aa-6850c46e940a")
	)
	(fp_line
		(start -1.25 -1.5)
		(end 7.75 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "03a85918-7e76-4cf5-a805-42385a23e829")
	)
	(fp_line
		(start 7.75 -1.5)
		(end 8 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0e920e14-089c-47ef-95d1-646ddeac4779")
	)
	(fp_line
		(start 7.75 6)
		(end -1.25 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5ce24ad0-407c-4dd4-a90d-8d5bbdd38ec4")
	)
	(fp_line
		(start 7.75 6)
		(end 8 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "93a44549-ff86-426a-829f-2e84e77ce4c9")
	)
	(fp_line
		(start 8 -1.5)
		(end 8 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6ca1ba81-9142-4671-947e-3924028aae73")
	)
	(fp_line
		(start 8 -1.25)
		(end 8 5.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eb91715c-9b35-46b4-9b63-fbd0275ad6b7")
	)
	(fp_line
		(start 8 6)
		(end 8 5.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "90537424-144e-4969-9b4d-e24d7e03a55d")
	)
	(fp_line
		(start 0.25 -0.75)
		(end 3.25 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6fdfeefe-a670-4219-8d25-fc00c80d0abd")
	)
	(fp_line
		(start 0.25 5.25)
		(end 0.25 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "05f7db50-10b8-4304-a362-8de27e084ea4")
	)
	(fp_line
		(start 3.25 -0.75)
		(end 6.25 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b0df6ce1-7218-41ab-b0f3-9f4411632bca")
	)
	(fp_line
		(start 6.25 -0.75)
		(end 6.25 5.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c07bc337-77cb-48a0-aa63-b5638149835f")
	)
	(fp_line
		(start 6.25 5.25)
		(end 0.25 5.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "278b64f2-92e6-483e-a8f1-22fbe6df86b3")
	)
	(fp_circle
		(center 3.25 2.25)
		(end 1.25 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "72096948-de13-4cec-9b66-353cacece6ba")
	)
	(fp_text user "${REFERENCE}"
		(at 3.25 2.25 0)
		(layer "F.Fab")
		(uuid "9a2dcefd-6c10-477d-9e8a-d464ccf12e84")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0 90)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "625b79d8-ebd4-4bd7-b795-bcf8f3408592")
	)
	(pad "1" thru_hole circle
		(at 6.5 0 90)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3618083d-c8da-4d5d-94ef-981e7c69da90")
	)
	(pad "2" thru_hole circle
		(at 0 4.5 90)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "83f737c8-f9c3-426f-9077-d5d1d6216183")
	)
	(pad "2" thru_hole circle
		(at 6.5 4.5 90)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "45a247b9-3755-4269-a049-947addc37dca")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
