(footprint "L_Taiyo-Yuden_NR-40xx"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-40xx, 4.0mmx4.0mm")
	(tags "inductor taiyo-yuden nr smd")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "7dd5fc5c-2f85-431a-81b1-e519bd1e5e7f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "6.8uH_1.0A_4018"
		(at 0 3.5 0)
		(layer "F.Fab")
		(uuid "9013e3eb-09a8-45d9-aa30-b91827cbc16b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "021a8df9-e511-4691-9c18-dc0ee9e53a6d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "6.8uH, Isat>1.4A, Idc>1.0A, Rdc<110mOhms, shielded"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "abe89c5e-b609-4bd4-81ce-577f1b103b63")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Specifications" "6.8uH, Isat>625mA, Idc>1.0A, Rdc<=100mOhms, shielded"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ad61b063-b57d-409a-8963-6a02576655c7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "Taiyo Yuden"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1fce88c-4c97-433d-af11-50e1beb9b8a9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part Number" "NRS4018T6R8MDGJ"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9fe2c209-f4fe-4bba-9db8-e0878a3de8d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Display" "6.8uH"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "411291de-e4db-4d3c-b3cd-684fac41dc1b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Display 2" "1.6A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d10b8390-e17f-4d6e-835a-26b4927498c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer 2" "Taiyo Yuden"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "80de54dd-399b-4b36-a447-877910e9a2b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part Number 2" "NRS4018T6R8MDGJV"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "24892cec-0b28-4a53-ac59-92cfb381871f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer 3" "Taiyo Yuden"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2cb0aa8-cd92-4e87-ac12-0e4ba52e762e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part Number 3" "NR4018T6R8M"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "052c4e60-2ef7-4561-a6a4-72782faa375d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer 4" "Bournes"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ae0e18db-b649-4d2e-a313-273539723453")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part Number 4" "SRN4018TA-6R8M"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "067388d2-be3b-41e8-a9e5-8b37669f3930")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer 5" "ABRACON"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "906a53e5-3eca-40e5-9bfc-e38d633b733c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part Number 5" "ASPI-0418FS-6R8M-T3"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "24f5fd95-1893-4f29-9ea4-033f588e0971")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB ID" "C223055"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ecb82fea-7dc3-4ea7-b89c-4430b0f743b0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2 -2.1)
		(end 2 -2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e67fc0c5-9fa7-4f5a-a632-d32818babe98")
	)
	(fp_line
		(start -2 2.1)
		(end 2 2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "587337b9-cb41-4dce-bb89-9b474cf7ccf9")
	)
	(fp_line
		(start -2.25 -2.25)
		(end -2.25 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c750537f-8997-4d0d-a423-f1fff4c958c8")
	)
	(fp_line
		(start -2.25 2.25)
		(end 2.25 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "82ba8c5f-88da-46aa-910b-1ea17c12ba6c")
	)
	(fp_line
		(start 2.25 -2.25)
		(end -2.25 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b7b8e89c-5f36-4d25-a18f-1700a9dcdd58")
	)
	(fp_line
		(start 2.25 2.25)
		(end 2.25 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1efe7db0-ac7b-4f30-b21c-fcd7bac304e1")
	)
	(fp_line
		(start -2 -1.25)
		(end -1.25 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "508ea34e-9ce6-4c94-a794-b1c6298c4f8a")
	)
	(fp_line
		(start -2 1.25)
		(end -2 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0bc2144d-a143-4605-8679-aff0003a4c34")
	)
	(fp_line
		(start -2 1.25)
		(end -1.25 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5da64bd8-d470-4f3b-8e81-5000e6f45f27")
	)
	(fp_line
		(start -1.25 -2)
		(end 1.25 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f4f24927-f454-4a7b-9ee5-340f5f093722")
	)
	(fp_line
		(start -1.25 2)
		(end 1.25 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "10c25f78-d127-4bd7-ac77-53f27c97b0b9")
	)
	(fp_line
		(start 2 -1.25)
		(end 1.25 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6f4a8fc3-2a59-4dd4-9a28-f2b0f2958311")
	)
	(fp_line
		(start 2 -1.25)
		(end 2 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1275f17d-7f75-4712-b4ac-75804701434c")
	)
	(fp_line
		(start 2 1.25)
		(end 1.25 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1e266121-68e9-4150-b4c3-f259d5e9ac3f")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1bb8e035-b457-4639-929d-4a6aae3c055d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -1.4 0)
		(size 1.2 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "aaef1a7b-1fb6-4c05-8514-d4ad2cb3fe59")
	)
	(pad "2" smd rect
		(at 1.4 0)
		(size 1.2 3.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "1a446019-6fe6-473a-9f3c-6f5634393971")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_NR-40xx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
