(footprint "C_1206_3216Metric"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "SparkFun capacitor")
	(property "Reference" "REF**"
		(at 0 -1.85 0)
		(layer "F.Fab")
		(uuid "50ca94fb-6743-4e90-bdf4-b5c9f8960a3d")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.1)
				(bold yes)
			)
		)
	)
	(property "Value" "22uF"
		(at 0 1.85 0)
		(layer "F.Fab")
		(uuid "e566b9f5-1c33-4527-b4f0-c8825b6490cc")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.1)
				(bold yes)
			)
		)
	)
	(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/658/CL31A106KBHNNNE_Spec.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2de982db-4797-4d3d-98b3-726638e56657")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Unpolarized capacitor"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fc10ace3-4ecf-4628-983a-5c39f5148717")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "PROD_ID" "CAP-15263"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "78734044-236a-4198-818e-fdc3c5b43aab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Voltage" "50V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e06231f-166a-4560-99a1-8d564dbfc6cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Tolerance" "10%"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3b41e49c-4a9d-4b97-bd3a-4cd1b558f534")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.711252 -0.91)
		(end 0.711252 -0.91)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a3aa55bf-fba0-401e-be3c-f8cc0ea8c309")
	)
	(fp_line
		(start -0.711252 0.91)
		(end 0.711252 0.91)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "128ee8c9-19af-466c-acf9-d2837dab667a")
	)
	(fp_line
		(start -2.3 -1.15)
		(end 2.3 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1790d13a-87c4-41d3-ba69-16dba50a00a3")
	)
	(fp_line
		(start -2.3 1.15)
		(end -2.3 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ec54e315-bcc2-45b6-b452-953ed4b531b5")
	)
	(fp_line
		(start 2.3 -1.15)
		(end 2.3 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6076f83f-1eb8-4ad3-8dc3-35f911c03d7c")
	)
	(fp_line
		(start 2.3 1.15)
		(end -2.3 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "08471aec-6c10-406a-a479-52b834256e58")
	)
	(fp_line
		(start -1.6 -0.8)
		(end 1.6 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "208fc851-914f-40da-81d1-247d4d3dd543")
	)
	(fp_line
		(start -1.6 0.8)
		(end -1.6 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b3f9453-dd0a-4abf-82a7-510e756b68fd")
	)
	(fp_line
		(start 1.6 -0.8)
		(end 1.6 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "abfcca99-a905-450e-a074-260aed148ef6")
	)
	(fp_line
		(start 1.6 0.8)
		(end -1.6 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "95fe3bf9-ef9d-4f24-8046-1c9fe9f1f5ef")
	)
	(pad "1" smd roundrect
		(at -1.475 0)
		(size 1.15 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "a5637dd0-e6c1-4fa3-9409-2d30c4c3277a")
	)
	(pad "2" smd roundrect
		(at 1.475 0)
		(size 1.15 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "7bd749ca-99b9-44af-829b-d9d0f77639e5")
	)
	(embedded_fonts no)
	(model "${KICAD9_3RD_PARTY}/3dmodels/com_github_sparkfun_SparkFun-KiCad-Libraries/Capacitor.3dshapes/C_1206_3216Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
